I started making a temporary .pka file that I will use for the CA.

Using the network “172.16.0.0/16” for the company **Corona Fightback Solution**.

Medical has 10 Application servers and Marketing has 5 application servers.

Everyone has access to a customized web server.

Subnets for all the departments.

VLANs for each department/subnet.

Security for all of the Routers and Switches. (such as line vty 0 4, enable password cisco, enable secret class, service password-encryption)

IP Addressing Scheme where I started by figuring out my subnets, unsure whether to use VLSM or not.

Subnetting